File E103521 Vol. l Sec. 1 Page lA Issued: 1986-11-06

and Report Revised: 2023-07-23

Conditions of Acceptability -

l. The transformers**, except otherwise noted,** are provided with a Class l05 insulation system.

The manufacturer claims that the insulating system is suitable for

120°C. UL has not evaluated the insulating system for this rating.

2. These components have been judged on the basis of the required spacing in the Standard for Electronic Data Processing Equipment (UL 478) which covers the end-use product for which the component was intended.

# Primary winding 400 V max. In regard to IEC 38 “IEC Standard Voltages”

3. Only FLN series are provided with a Class 130B insulation System **OBJY2** (E216803).