|  |  |  |
| --- | --- | --- |
| **Issued to:** |  | BLOCK TRANSFORMATOREN-ELEKTRONIK GMBH |
| MAX-PLANCK-STRASSE 36-46  27308 VERDEN GERMANY |
|  |  |  |
| **This is to certify that**  **representative samples of** |  | COMPONENT - POWER CIRCUIT AND MOTOR-MOUNTED APPARATUS |
| See Addendum Page |
|  |  |  |
|  |  | Have been investigated by UL in accordance with the Standard(s) indicated on this Certificate. |
|  |  |  |
| **Standard(s) for Safety:** |  | UL508, Industrial Control Equipment  CSA C22.2 No. 14, Industrial Control Equipment |
| **Additional Information:** |  | See the UL Online Certifications Directory at [www.ul.com/database](http://www.ul.com/database) for additional information |

­­­

Only those products bearing the UL Recognized Component Marks for the U.S. and Canada should be considered as being covered by UL's Recognition and Follow-Up Service and meeting the appropriate U.S. and Canadian requirements.

The UL Recognized Component Mark for the U.S. generally consists of the manufacturer’s identification and catalog number, model number or other product designation as specified under “Marking” for the particular Recognition as published in the appropriate UL Directory. As a supplementary means of identifying products that have been produced under UL’s Component Recognition Program, UL’s Recognized Component Mark: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: RU1, may be used in conjunction with the required Recognized Marks. The Recognized Component Mark is required when specified in the UL Directory preceding the recognitions or under “Markings” for the individual recognitions. The UL Recognized Component Mark for Canada consists of the UL Recognized Mark for Canada: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: Description: CRU1 and the manufacturer’s identification and catalog number, model number or other product designation as specified under “Marking” for the particular Recognition as published in the appropriate UL Directory.

Recognized components are incomplete in certain constructional features or restricted in performance capabilities and are intended for use as components of complete equipment submitted for investigation rather than for direct separate installation in the field. The final acceptance of the component is dependent upon its installation and use in complete equipment submitted to UL LLC.

Look for the UL Recognized Component Mark on the product.

This is to certify that representative samples of the product as specified on this certificate were tested according to the current UL requirements.

Open type reactors for use as inverter (AC drive) output filters and chokes, series SFB and MDB or 6SE6400, 6SL3000 followed by any letters or digits.

Open type reactors for use as inverter (AC drive) line input chokes, series NKD, NKE or B or 6SE6400 or 6SL3203, followed by any letters or digits