File E103521 Vol. 1 Sec. 3 Page 2 Issued: 1997-03-31

 and Report Revised: 2005-05-19

CONDITIONS OF ACCEPTABILITY:

 1. The transformers and reactors type EI, UI and 3UI are provided

with a

 - class 105 insulation system (core term code suffix A)

 or

 - class 130 insulation system (core term code suffix B)

 or

 - class 155 insulation system (core term code suffix F)

 **or**

 **- class 180 insulation system (core term code suffix H1)**

 The transformer type B9904048 is provided with class 130 insulation system designated B1 (see table II) or B2 (see table III)